formZ SDK | 5.0 API Reference | Project | Modeling | Attributes

# fz_objt_attr_rmsh_copy

Description

Copy the content of one radiosity meshing attribute to another. Note, that the destination radiosity meshing must already be allocated. This can be done by a call to fz_objt_attr_rmsh_init.

Plugin Prototype

fzrt_error_td fz_objt_attr_rmsh_copy(

fzrt_int | src_windex,
fz_attr_rmsh_ptr | src_rmsh,
fzrt_int | dst_windex,
fz_attr_rmsh_ptr | dst_rmsh )

Parameters

src_windex [Input]

source project

src_rmsh [Input]

source attribute

dst_windex [Input]

destination project

dst_rmsh [Input]

destination attribute

Returns

Error codes

Availability

5.0.0.0

Example Files

util_attr_rmsh.fsl

See Also

fz_objt_attr_rmsh_init,,, fz_objt_attr_rmsh_finit

Function Set

fz_objt_attr_fset

Defined in

fz_objt_attr_api.h