formZ SDK | 5.0 API Reference | Project | Modeling | View Manager

# fz_view_camera_std_enum

Description

Standard predefined camera types.

enum fz_view_camera_std_enum {

FZ_VIEW_CAMR_STD_HALF,

FZ_VIEW_CAMR_STD_FULL,

FZ_VIEW_CAMR_STD_NTSC,

FZ_VIEW_CAMR_STD_NTSA,

FZ_VIEW_CAMR_STD_PALL,

FZ_VIEW_CAMR_STD_SVGA,

FZ_VIEW_CAMR_STD_17IN,

FZ_VIEW_CAMR_STD_35MM,

FZ_VIEW_CAMR_STD_70MM,

FZ_VIEW_CAMR_STD_HDT1,

FZ_VIEW_CAMR_STD_HDT2,

FZ_VIEW_CAMR_STD_SXGA,

FZ_VIEW_CAMR_STD_NTS2 };

Members

FZ_VIEW_CAMR_STD_HALF

Half Screen - (320 x 240 pixel aspect = 1.0 aspect = 4./3. )

FZ_VIEW_CAMR_STD_FULL

Full Screen (VGA) - (640 x 480 pixel aspect = 1.0 aspect = 4./3. )

FZ_VIEW_CAMR_STD_NTSC

NTSC - (720 x 486 pixel aspect = 0.9 aspect = 4./3. )

FZ_VIEW_CAMR_STD_NTSA

NTSC (Width Adj.) - (648 x 486 pixel aspect = 1.0 aspect = 4./3. )

FZ_VIEW_CAMR_STD_PALL

PAL - (768 x 576 pixel aspect = 1.0 aspect = 4./3. )

FZ_VIEW_CAMR_STD_SVGA

SVGA, - (800 x 600 pixel aspect = 1.0 aspect = 4./3. )

FZ_VIEW_CAMR_STD_17IN

Large Screen (XGA) - (1024 x 768 pixel aspect = 1.0 aspect = 4./3. )

FZ_VIEW_CAMR_STD_35MM

35mm Slide Film - (3072 x 2048 pixel aspect = 1.0 aspect = 3./2. )

FZ_VIEW_CAMR_STD_70MM

70mm Film - (2130 x 1152 pixel aspect = 1.0 aspect = 1.85 )

FZ_VIEW_CAMR_STD_HDT1

HDTV (Low Res) - (1280 x 720 pixel aspect = 1.0 aspect = 16./9.)

FZ_VIEW_CAMR_STD_HDT2

HDTV (High Res) - (1920 x 1080 pixel aspect = 1.0 aspect = 16./9.)

FZ_VIEW_CAMR_STD_SXGA

Super XGA - (1280 x 960 pixel aspect = 1.0 aspect = 4./3. )

FZ_VIEW_CAMR_STD_NTS2

NTSC (Height Adj.) - (720 x 540 pixel aspect = 1.0 aspect = 4./3. )

Availability

5.0.0.0

Defined in

fz_view_api.h