formZ SDK | 5.0 API Reference | Project | Modeling | Objects | Plain Object Construction

# fz_objt_cnstr_fillet

Description

Creates a fillet surface between the two input faces. The source objects must be either surfaces or solids. The faces between which a fillet surface needs to be constructed are specified by their indices. The parameter do_convex specifies whether a convex or a concave fillet is requested. If do_basic is TRUE then radius is used else srnd_opts is used for the cross-section of fillet surface. An approximate starting point for fillet surface needs to be specified.

Plugin Prototype

fzrt_error_td fz_objt_cnstr_fillet(

fzrt_int | windex,
fz_objt_ptr | src_obj1,
fzrt_int | findx1,
fz_objt_ptr | src_obj2,
fzrt_int | findx2,
fzrt_boolean | do_convex,
fzrt_boolean | do_basic,
double | radius,
fz_objt_srnd_opts_ptr | srnd_opts,
fz_xyz_td * | start_pt,
fz_attr_refn_ptr | refn_opts,
fz_objt_ptr * | obj )

Parameters

windex [Input]

project window index

src_obj1 [Input]

Source object 1

findx1 [Input]

Face index 1

src_obj2 [Input]

Source object 2

findx2 [Input]

Face index 2

do_convex [Input]

TRUE=Convex/FALSE=Concave

do_basic [Input]

TRUE=Basic/FALSE=Advanced

radius [Input, Optional]

Radius- Applicable only if do_basic is TRUE

srnd_opts [Input, Optional]

Advanced options- Applicable only if do_basic is FALSE

start_pt [Input]

Approximate starting point

refn_opts [Input]

obj [Result]

New object

Returns

Error codes

Availability

5.0.0.0

Example Files

util_objt_filt.fsl

Function Set

fz_model_fset

Defined in

fz_objt_filt_api.h