formZ SDK | 5.0 API Reference | Project | Modeling | Attributes

# fz_attr_rmsh_parm_enum

Description

radiosity meshing parameters ids. Used to set/get the parameters of a radiosity meshing attribute using and

enum fz_attr_rmsh_parm_enum {

FZ_ATTR_RMSH_PARM_MESH_ON,

FZ_ATTR_RMSH_PARM_PATCHES,

FZ_ATTR_RMSH_PARM_POLYS,

FZ_ATTR_RMSH_PARM_ADAPT_ON,

FZ_ATTR_RMSH_PARM_ADAPT_DENSITY,

FZ_ATTR_RMSH_PARM_ADAPT_THRESSHOLD };

Members

FZ_ATTR_RMSH_PARM_MESH_ON

radiosity meshing is on/off

Type: fzrt_boolean

Default Value: FALSE

FZ_ATTR_RMSH_PARM_PATCHES

density of radiosity patches. The normal range is from 0.0 to 1.0, but values larger than 1.0 can be used.

Type: double

Default Value: 0.5

Range: value > 0.0

FZ_ATTR_RMSH_PARM_POLYS

# of radioslity mesh polygons as a factor of the number of radiosity patches.

Type: double

Default Value: 5.0

Range: value > 0.0

FZ_ATTR_RMSH_PARM_ADAPT_ON

adaptive radiosity meshing is on

Type: fzrt_boolean

Default Value: FALSE

FZ_ATTR_RMSH_PARM_ADAPT_DENSITY

density of adaptive meshing.

Type: double

Default Value: 0.8

Range: 0.0 <= value <= 1.0

FZ_ATTR_RMSH_PARM_ADAPT_THRESSHOLD

threshold of adaptive meshing.

Type: double

Default Value: 0.2

Range: 0.0 <= value <= 1.0

Availability

5.0.0.0

See Also

,

Defined in

fz_objt_attr_api.h