formZ SDK | 5.0 API Reference | System | Nurbs Curve

# fz_ncrv_merge_align

Description

Merges two NURBS curves using alignment.

Plugin Prototype

fzrt_error_td fz_ncrv_merge_align(

fz_nurbs_cur_ptr | crv1,
fz_nurbs_cur_ptr | crv2,
fz_nurbs_algn_type_enum | align_type,
fz_nurbs_cur_ptr * | merge_crv )

Parameters

crv1 [Input]

NURBS curve 1

crv2 [Input]

NURBS curve 2

align_type [Input]

alignment type when smooth curves is FALSE (C0, G1, C1, C2)

merge_crv [Result]

NURBS curve

Returns

Error codes

Availability

5.0.0.0

Example Files

util_ncrv.fsl

Function Set

fz_ncrv_fset

Defined in

fz_ncrv_api.h