formZ SDK | 5.0 API Reference | System | Runtime Library (FZRT) | Memory

# fzrt_endian_swap_ulong

Description

Swaps byte order of an fzrt_unsigned_int integer. This is useful for switching between endian byte order of a fzrt_int integer

Plugin Prototype

fzrt_error_td fzrt_endian_swap_ulong(

fzrt_unsigned_int * | data )

Parameters

data [Input, Result]

pointer to fzrt_unsigned_int to swap, contains swapped value on exit

Returns

FZRT_NOERR on success, otherwise an error ID

Availability

5.0.0.0

See Also

fzrt_endian_swap_4_bytes,

Function Set

fz_fzrt_mem_fset

Defined in

fzrt_api.h