formZ SDK | 5.0 API Reference | Project | Modeling | Objects | Editing Operations

# fz_objt_edit_split_with_line

Description

Splits object 1 with object 2.
Object 2 must be an open or closed, planar wire. norm indicates the direction along which the cutting wire is projected. As it is possible that more than one object is created, the pointers of the resulting objects are stored in the entity list passed in.

Plugin Prototype

fzrt_error_td fz_objt_edit_split_with_line(

fzrt_int | windex,
fz_objt_ptr | obj1,
fz_objt_ptr | obj2,
fz_xyz_td * | norm,
fzrt_boolean | join_volumes,
fz_enty_list_ptr | ent_list )

Parameters

windex [Input]

project window index

obj1 [Input]

object 1

obj2 [Input]

object 2 (must be an open or closed planar wire)

norm [Input]

indicates the direction along which the cutting wire is projected

join_volumes [Input]

If set to TRUE, all resulting volumes will be joined into one object. Otherwise, one object per volume will be created.

ent_list [Result]

list with new object pointers

Returns

Error codes

Availability

5.0.0.0

Example Files

util_objt_split_stitch.fsl

See Also

,,,, fz_objt_edit_trim_with_surface,,, fz_objt_edit_stitch_faces,, , fz_objt_edit_section3d, fz_objt_edit_section2d, fz_objt_edit_volumes_join,

Function Set

fz_model_fset

Defined in

fz_objt_api.h