formZ SDK | 5.0 API Reference | System | Data Type

# fz_type_get_ulong

Description

This function performs the following data type conversions:
Variant Type Conversion
fzrt_boolean TRUE -> 1; FALSE -> 0.
char value clamped to range of 0 to 127.
unsigned char value copied, no data lost.
short value clamped to range of 0 to 32767.
unsigned short value copied, no data lost.
fzrt_int bits copied, value < 0 wrap to range of -(2^31) to 0.
float value converted to integer then clamped to range of 0 to (2^32)-1.
double value converted to integer then clamped to range of 0 to (2^32)-1.

Plugin Prototype

fzrt_error_td fz_type_get_ulong(

fz_type_ptr | type,
fzrt_unsigned_int * | lval )

Parameters

type [Input]

A pointer to a variant

lval [Result]

A pointer to a value to be filled. Must be allocated by the caller.

Availability

5.0.0.0

See Also

, fz_type_get_ulong_ptr

Function Set

fz_type_fset

Defined in

fz_type_api.h